# System-Wide Traffic Prioritization with IEEE-802.1p

- ## 802.1p support available for NICs today (Windows/nT)

- ## Layer 2 Switches with multiple hardware queues for 802.1p available today

- ## Layer 3 Switches with 802.1p and RSVP support available today

- ## Total end-to-end Traffic Prioritization available today

802.1p/Q

Enabled NIC

Tagged Frame

Priority

Queues

1

2

3

L3 Switch: Maps

Tag to Queue

L2 Switch:

802.1p/Q

4

Central policy-setting tools are emerging

Previous slide | Next slide | Back to first slide | View graphic version