# Admission Control for Bandwidth Reservation and Security

- Manage Security and Firewalls at linespeed
  - Traffic classifiers to restrict identified flows
  - Built-in filters
    - Port Group filter, MAC Group filter, Combination (MAC Address & Dest. Port)
    - Protocol Type Filter
    - IP Flow filters
  - Broadcast/Multicast containment
    - By VLAN, MAC address, port, protocol, ...

- Bandwidth Reservation
  - Use traffic classifiers to allocate bandwidth to identified flows
  - Static
  - Dynamic
  - RSVP

Previous slide | Next slide | Back to first slide | View graphic version