# Admission Control:
User Defined Filters

- ## User defined filtering

  - Programmable up to 64 bytes into packet
  - Multiple filtering paths (TxA,TxM,RxA,RxM) per port for optimal performance
  - Filtering IP directed broadcasts (Internet2)

- ## ASIC accelerated

  - Secure Address groups
  - Firewalling
  - User defined policies between ports or groups
  - Advertisement filters

- ## MIB support for packet filters

Previous slide | Next slide | Back to first slide | View graphic version